**(1) Species:**maple veneer

**(2)** **Application**: applied to the surface of the furniture & door. It is also commonly used in surface of plywood, MDF, chipboard and interior decoration, etc

**(3) MOQ:** 2000.00 m2.

**(4) Terms of payment:** TT, LC at sight.

**(5) Delivery date:** within 7-15 days after order confirmed.

**(6) VicWin wood also accept your special order.**

|  |  |
| --- | --- |
| **Length** | **1300mm up, 2000mm up, 2500mm up** |
| **Width** | **120mm up** |
| **Thickness** | **0.3mm/0.5mm** |
| **Grain** | **C/C & Q/C** |
| **Grade** | **Furniture/Door/Panel** |

VicWin Wood consistently focus on veneer quality. Our QC aim is to create the need for constant expansion to keep up with ever-increasing demand.

**Species**: American walnut veneer, white oak veneer, red oak veneer, cherry veneer, sapwood veneer, knotty oak veneer, santos rosewood veneer, white ash veneer/American ash veneer, maple veneer, prima vera veneer, knotty ash veneer, birds eye maple veneer, olive ash veneer.